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United Nations Population Fund, 

UNFPA Yemen

Haddah St. behind Lazourde Hotel 

Sanaa’a.,Yemen

Tel: +967 1 433160 

Website: www.unfpa.org
Email:procurement.yemen@unfpa.org 

Date: 06/07/2026
Request for Quotation No. YEM/2026/003
Provision of Security items for UNFPA 
Dear Sir/Madam, 

We hereby solicit your quotation for the supply of X-ray and metal detector for UNFPA- Aden office, as per the technical specifications detailed in Annex I of this RFQ. 

The items are to be delivered to Aden as within three weeks from PO issuance.  The quotation shall be valid at least for 3 months after the closing date.
If you are interested in submitting a quotation for these services, kindly fill in the attached Quotation Form or your Company form and send by E-mail only to the address indicated below not later than 12/07/2026, 14:00 (Aden time):
Email: procurement.yemen@unfpa.org  

Bidders must enter the following text in the email subject line:
RFQ/YEM/2026/003 – Security Items 
Please submit your quotation in US Dollars currency. Conversion of currency into the UNFPA preferred currency, if the offer is quoted differently from what is required, should be based only on UN Operational Exchange Rate prevailing at the time of competition deadline. 
For any technical inquiries, please contact bisher@unfpa.org
Bidders should NOT submit any Bid to this contact or your Bid will be declared invalid, as UNFPA will not able to guarantee the confidentiality of the Bidding process.

Bidders may request clarifications not later than 10 July 2026, 14:00 Aden time.

Quotations submitted by email must be free from any form of virus or corrupted contents, or the quotations shall be rejected.  

It shall remain your responsibility to ensure that your quotation will reach the address above on or before the deadline. Quotations that are received by UNFPA after the deadline indicated above, for whatever reason, shall not be considered for evaluation. Kindly ensure that it is signed and in the .PDF format, and free from any virus or corrupted files.

Please take note of the following requirements and conditions pertaining to the supply of the above mentioned goods:
Partial quotes - Not Permitted

Partial delivery – Not Permitted

Alternative Bids are not accepted under this RFQ. In the event of a supplier submitting more than one bid, the following shall apply:

· All bids marked alternative will be rejected and only the base will be evaluated; 

· All bids will be rejected if no indication is provided as to which bids are alternative bids.

Bidders may modify their offers in writing prior to the submission deadline. The bidder must submit the proposed modification via email that must be clearly marked as “MODIFICATION”.

In this case, the previous offer will be declined and the modified offer shall be considered for the evaluation process.  Also, if the same bidder has submitted several offers before the bid deadline superseding each other only the last received offer will be considered for opening and further evaluation.
Note: Current UNFPA supplier policies apply to this solicitation and can be found at: http://www.unfpa.org/suppliers.
Documents to be submitted with the bid:
a. Duly Completed and Signed Bid Submission Form

b. Duly Completed and Signed Financial bid form
c. Duly Completed – Delivery Schedule Form 

d. Evidence of previous experience in a similar field and with the same type of requirements: list of major contracts completed within the last three years with national, international organizations, including UN. 

e. Latest Business Registration Certificate, (please note that all registration documents and licenses must be valid);
f. Latest Internal Revenue Certificate / Tax Clearance;  

Best regards,

UNFPA 

Yemen

Quotation Form
Name of Bidder:









Date of Bid:










Request for Quotation No:








Currency of Bid price:









Delivery time (weeks from receipt of order till dispatch):




Expiration of Validity of Quotation (The quotation shall be 

valid for a period of at least 3 months after the Closing date.):




Price Schedule:

	Item No.
	Quantity
	Transportation cost to port of Destination (specify mode of trp.)
	Total CPT/CFR (Destination port)
	Delivery schedule (months)

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


In your offer, please include:

1. Specific technical specifications of products offered
2. Quality standard of the products


I hereby certify that this company, which I am duly authorized to sign for, accepts the terms and conditions of UNFPA (http://www.unfpa.org/resources/unfpa-general-conditions-contract ) and we will abide by this quotation until it expires. 

Name and title







Date and Place
Annex I
SECTION 1: Technical Specifications

1.1 Professional X-Ray Baggage Scanner (Quantity: 1 Unit)

The required equipment must be a commercial-grade X-ray baggage scanner featuring an inspection tunnel that measures at least 600 mm wide by 400 mm high. To ensure highly accurate screening, the scanner must utilize advanced dual-energy imaging technology. This system must automatically separate and color-code materials on the operator's screen, clearly distinguishing between organic materials like explosives or narcotics, inorganic items like metals, and complex mixed or threat objects. Additionally, we prefer systems equipped with an automated threat detection platform driven by AI or advanced algorithms(if possible). This software must provide real-time assistance by automatically identifying, framing, and highlighting suspicious items or anomalies such as weapons, liquid threats, and explosives.

From a performance and safety standpoint, the X-ray beam must be powerful enough to guarantee a minimum steel penetration of 35 mm. The entire machine must strictly comply with established international radiation safety standards, such as FDA CFR 21 1020.40 or CE benchmarks, ensuring that stray radiation levels remain safely below legal limits for daily operators. For power reliability, the scanner must connect to a dedicated, line-interactive Online Uninterruptible Power Supply (UPS) supplied by the vendor. This backup battery must be capable of providing at least 30 minutes of continuous operational power if the primary electricity fails. The setup must also feature a built-in automatic transfer switch or communication link that instantly shifts the machine over to the facility’s backup power grid without causing the system to drop, reboot, or interrupt active scanning.

1.2 Walk-Through Metal Detector - WTMD (Quantity: 1 Unit)

The walk-through metal detector must feature a multi-zone pinpoint detection layout with at least 3 independent vertical zones to accurately pinpoint the location of hidden metallic objects from head to toe. The detector's inner software must come pre-loaded with standard international discrimination programs designed to meet safety benchmarks across varied environments.

It needs to run on microprocessor-based digital circuitry to maximize stability and minimize frustrating false alarms caused by environmental interference. For smooth traffic flow, the unit must include clear LED pacing lights on the frame to signal when a person should stop or proceed, alongside high-volume audible alarms that can be manually adjusted for volume. Finally, the unit must strictly meet the established NIJ 0601.02 security standard for walk-through metal detectors.

SECTION 2: Vendor Qualifications & Local Support Requirements

Because keeping this security equipment operational at all times is vital, vendors must fulfill strict support requirements directly inside Yemen. Bidders must provide a minimum of a two-year comprehensive, on-site warranty that completely covers all replacement parts, repair labor, necessary preventive maintenance visits, and routine software updates, including essential updates to the threat library used by the X-ray's automatic detection software. To back this up, the vendor must supply certified, documented proof that they have qualified field technicians permanently living and working in Yemen who can be deployed quickly for repairs. Bidders must also explicitly guarantee and document that they maintain a local inventory of critical spare parts within Yemen, ensuring that machine downtime is restricted to a maximum threshold of 48 to 72 hours throughout the entire warranty window.

SECTION 3: Mandatory Training Services

The chosen vendor is required to deliver structured, certified training programs on-site . Bidders must include a clear training timeline and curriculum that addresses two distinct learning tracks.

The first track is the X-Ray Operator Proficiency Training, which is designed for frontline security screeners and machine operators. This course focuses on basic and intermediate daily workflows, teaching staff how to read X-ray images, analyze color-coded materials, and identify threats. It must also teach operators how to use image tools like zoom, high-penetration mode, edge enhancement, and inverse imaging, while covering emergency shutdown steps and basic radiation safety before concluding with a practical evaluation and formal user certification.

The second track is the Advanced Administration Training, which targets security staff and Information & Communications Technology (ICT) staff. This advanced curriculum must cover software administration, deeper system changes, and first-line hardware fixes. For security management, it must detail user account management, access rights, audit logs, and reports. For software maintenance, it must cover adjusting algorithmic sensitivity matrices and updating threat libraries. On the tech side, ICT personnel must learn network configuration, data backup routines, image archive extraction, and power-flow management through the UPS and transfer switch. Finally, it must teach staff basic hardware calibration, error-code troubleshooting, and regular preventive maintenance routines.

Vendor’s Comments:
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